# TM/BA Series Printer Driver for Linux
TM-U375 Slip Model Manual

## Contents

1. Preface
2. Overview
3. Initial settings
4. Setting values of printing options
5. Paper size information
6. Restrictions

## 1. Preface

This manual describes printing conditions you can specify when printing on a TM-U375 Slip with "TM/BA Series Printer Driver for Linux."

Refer to the driver manual for information on "TM/BA Series Printer Driver for Linux."

## 2. Overview

The TM-U375 Slip uses the "TM Slip" of the TM generic model.

-The model name to choose when adding a printer by CUPS WebAdmin:
"EPSON TM Slip (rastertotmu) (en)"

-A corresponding PPD file:
tm-slip-rastertotmu.ppd

You can specify the following printing options for the TM-U375 Slip.

Setting value | CUPS Admin display | Description
--- | --- | ---
PageSize | Media Size | Paper size
TmxPaperReduction | Paper Reduction | Blank page saving
TmxPaperSource | Paper Source | Whether to cut or feed the
TmxEjectDirection | Eject Direction | Eject direction
TmxPrinterType | Printer Type | Printer type
Resolution | Resolution | Output resolution
TmxFeedPitch | Pitch of Feed | Unit length of a paper feed
TmxMaxBandWidth | Maximum Band Width | Maximum image width
TmxBandLines | Band Lines | Band Height for image command
TmxBidirectionalPrinting | Printing | Bidirectional printing
TmxDrawerControl | Cash Drawer | Cash drawer control
TmxPulseOnTime | Pulse On Time | Pulse width of cash drawer kick

Setting values of printing options can be changed from the GUI or the command line. For descriptions on setting values of each print option, see "4. Setting values of printing options."

Example) Specify the paper size to Cut sheet (230 x 297 mm) using an lp command.
$ lp -o Pagesize=CS230x297

Note)

! You can also specify the number of copies using a CUPS’ proprietary option.
Refer to the CUPS document for information on CUPS’ proprietary options.

http://localhost:631/help/

## 3. Initial settings

Initial settings of the printer options are as follows.
The mark (*) shows a different option from the initial value of a driver.
Please be careful on setting the option marked with (*).

CUPS Admin display | Initial setting
--- | ---
[General]
Cut sheet 182 x 257 mm (*)
None
Cut sheet [Eject]
Feed direction
[Printer Setting]
Impact slip
160 x 144 dpi
144 dpi
400 (*)
8
Bidirectional
[Cash Drawer Control]
Don’t open drawers
20 msec

## 4. Setting values of printing options

The following settings are available in printing options.

### [General]

Media Size: Specify the paper size

Setting value | CUPS Admin display | Description
--- | --- | ---
CS230x297 | Cut sheet 230 x 297 mm | <Unselectable>
CS182x257 | Cut sheet 182 x 257 mm | Cut sheet (182 x 257 mm)
A4 | A4 | <Unselectable>
LT | LT | <Unselectable>

Paper Reduction: Specify whether to save blank pages

Setting value | CUPS Admin display | Description
--- | --- | ---
Off | None | Do not save blank pages
Top | Top margin | Save blank at the top
Bottom | Bottom margin | Save blank at the bottom
Both | Top & Bottom margins | Save blank at the top and bottom

Paper Source: Specify whether to cut or feed the paper

Setting value | CUPS Admin display | Description
--- | --- | ---
SheetEject | Cut sheet [Eject] | Eject the paper after print
SheetNoEject | Cut sheet [NoEject] | Don’t eject the paper

Eject Direction: Specify the eject direction

Setting value | CUPS Admin display | Description
--- | --- | ---
FeedDirection | Feed direction | Eject paper to the feed direction
ReverseFeedDirection | Reverse feed direction | <Unselectable>

### [Printer Setting]

Printer Type: Specify the printer type

Setting value | CUPS Admin display | Description
--- | --- | ---
ImpactSlip | Impact slip | Impact slip type

Resolution: Specify the output resolution

Setting value | CUPS Admin display | Description
--- | --- | ---
80x72dpi | 80 x 72 dpi | Output at 80 x 72 dpi
160x144dpi | 160 x 144 dpi | Output at 160 x 144 dpi
144x130dpi | [90%/160x144dpi] | 90% reduced (160x144dpi)
128x115dpi | [80%/160x144dpi] | 80% reduced (160x144dpi)
112x101dpi | [70%/160x144dpi] | 70% reduced (160x144dpi)
96x86dpi | [60%/160x144dpi] | 60% reduced (160x144dpi)
82x73dpi | [50%/160x144dpi] | 50% reduced (160x144dpi)
72x65dpi | [45%(A4 to 85mm)/160x144dpi] | 45% reduced(A4 to 85mm) (160x144dpi)

Pitch of Feed: Specify the unit length of a paper feed

Setting value | CUPS Admin display | Description
--- | --- | ---
144.0 | 144 dpi | Paper feed at 144 dpi

Maximum Band Width: Specify the maximum image width

Setting value | CUPS Admin display | Description
--- | --- | ---
400 | 400 | 400 dots
540 | 540 | <Unselectable>

Band Lines: Specify the band height for image command

Setting value | CUPS Admin display | Description
--- | --- | ---
8 | 8 | Output band by 8 lines

Printing: Specify whether to print bidirectionally

Setting value | CUPS Admin display | Description
--- | --- | ---
Bidirectional | Bidirectional | Print bidirectionally
Unidirectional | Unidirectional | Print unidirectionally

### [Cash Drawer Control]

Cash Drawer: Specify the operation of cash drawer

Setting value | CUPS Admin display | Description
--- | --- | ---
None | Don’t open drawers | Do not open the drawer
Drawer#1,Before | Open drawer #1 BEFORE printing | Open drawer #1 before printing
Drawer#1,After | Open drawer #1 AFTER printing | Open drawer #1 after printing
Drawer#2,Before | Open drawer #2 BEFORE printing | Open drawer #2 before printing
Drawer#2,After | Open drawer #2 AFTER printing | Open drawer #2 after printing

Pulse On Time: Specify the pulse width of drawer kick

Setting value | CUPS Admin display | Description
--- | --- | ---
20,10,100 | 20 msec | On:20 msec, Off:200 msec
40,20,100 | 40 msec | On:40 msec, Off:200 msec
60,30,120 | 60 msec | On:60 msec, Off:240 msec
80,40,160 | 80 msec | On:80 msec, Off:320 msec
100,50,200 | 100 msec | On:100 msec, Off:400 msec
120,60,240 | 120 msec | On:120 msec, Off:480 msec

## 5. Paper size information

Paper size name | Input size | Margin | Output paper size
--- | --- | --- | ---
(CUPS Admin display) | Width | Length | Left | Right | Top | Bottom | Width | Length
| (mm) | (mm) | (mm)
Cut sheet 182 x 257 mm | 63.1 | 250.1 | 0.0 | 0.0 | 0.0 | 0.0 | 63.1 | 250.1

This driver allows you to specify the paper size using CUPS’ options.

Example) Print a file to 60 x 85 mm in size.
$ lp -o media=Custom.60x85mm file

The paper size can be specified within the following range.

Paper width: | 25.4 - 63.1 mm
Paper length: | 25.4 - 273.6 mm

## 6. Restrictions

* You cannot specify printing conditions for each page.

Copyright (C) Seiko Epson Corporation 2013-2015. All rights reserved.
Linux is the registered trademark or trademark of Linus Torvalds in the U.S.A. and other countries.
CUPS and the CUPS logo are trademarks of Apple Inc. registered in the U.S.A. and other countries.
Other product names in this document are trademarks or registered trademarks of respective companies.